|  |  |  |
| --- | --- | --- |
| ABRASIVE CLEAN & PAINT | To clean mechanically with abrasive grit or shot and paint | AB |
| CHEMICAL CLEAN | To clean a component with chemical wash | CC |
| FREE | To free a frozen, seized or stiff component by means of force, lubrications or heat | FR |
| INSERT | To remove & replace part of the cross sectional profile of a component over its entire length and/or width. The replacement portion is butt welded to the original component | IT |
| OVERLAPPING PARTIAL SECTION | To remove & replace part of the cross sectional profile of a component over its entire length and/or width. The replacement portion is overlapped with and fillet welded to the original component. The exterior of the patch is continuously welded to original component. The interior may be continuously or skip welded with sealer applied to the seems between skip welds. | OP |
| PAINT | To apply paint | PA |
| PATCH | To remove & replace a part of the cross sectional profiles of a component, over only part of the component's length and/or width. A patch is overlapped with and fillet welded to the original component. The exterior of the patch is continuously welded to original component. The interior may be contiuously or skip welded with sealer applied to the seems between skip welds. | PT |
| PREVENTIVE MAINTENANCE | Maintenance carried out under the owner's instructions | VM |
| RE-ALIGN | To remove or unfasten a component, usually doors, and refit to bring into alignment | RA |
| REFIT | To refit a removeable component to its proper position | FT |
| REPAIRS PRIOR TO REFURBISHMENT | Repairs ordered by owner prior to refurbishment | PV |
| REMOVE | a). To remove unwanted labels, marks, logos, graffiti and b) To remove and not replace any component | MV |
| REMOVE & REFIT | To remove & refit after repair | RR |
| REPLACE | Remove & replace the complete cross sectional profile of a component over its entire length & width | RP |
| SEAL | a). To repair pin holes in a tarpaulin cover or tilt using sealant b). To apply sealant to or around component | SE |
| SECTION | To remove & replace the component the complete cross sectional profile of a component over part of its length and/or width | SN |
| STRAIGHTEN | To repair by straightening | GS |
| STRAIGHTEN & RESECURE | To repair by straightening and securing the component when repaired | RS |
| STRAIGHTEN & WELD | To repair by straightening a component and rewelding it into position | GW |
| STEAM CLEAN | To clean the component, usually the floor, using high pressure steam | SC |
| SURFACE PREPARATION & PAINT | To clean & prepare the surface & apply paint | PS |
| SWEEP | To clean the component, usually the floor, by sweeping | WP |
| WATER WASH | To clean the component, usually the floor, using floor | WW |
| WELD | To repair by welding | WD |